Back to Contents

# Specifications: Intel PRO/Wireless 2915ABG Network Connection User Guide

- Intel PRO/Wireless 2915ABG Network Connection
- Intel PRO/Wireless 2200BG Network Connection

## Specifications: Intel PRO/Wireless 2915ABG Network Connection

Form Factor | Mini PCI Type 3A
Dimensions | Width 2.85 in x Length 1.75 in x Height 0.20 in (59.75 mm x 50.95 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin SO-DIMM edge connector
Voltage | 3.3 Volt
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz to 5.85 GHz | 2.400 - 2.472 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 non-overlapping, dependent on country | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Windows XP, Windows 2000
Wi-FiŽ Alliance certification | Wi-FiŽ certification for 802.11b, 802.11g, 802.11a
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA, WPA-Enterprise, AES 128-bit, WEP 128-bit and 64-bit.Cisco Compatible Extensions v2.0, 802.1x: LEAP, PEAP, TKIP, EAP-TLS, EAP-TTLS, MD5
Product Safety | UL, C-UL, CB (IEC 60590)

## Specifications: Intel PRO/Wireless 2200BG Network Connection

Form Factor | Mini PCI Type 3A
Dimensions | Width 2.85 in x Length 1.75 in x Height 0.20 in (59.75 mm x 50.95 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin SO-DIMM edge connector
Voltage | 3.3 Volt
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50 to 85% non-condensing
2.4 GHz Band (802.11b/g | Most of the World (United States) | Rest of World (Europe, Japan)
Frequency ranges | 2.412 - 2.462 GHz | 2.412 - 2.472 GHz
Channels | 1 - 11 (active scan) | 1 - 13 (active scan)
Modulation | CCK, DQPSK, DBPSK, BPSK, QPSK, 16 QAM, 64 QAM
Wireless Medium | 2.4 GHz ISM: Direct Sequence Spread Spectrum (DSSS) and Orthogonal Frequency Division Multiplexing (OFDM)
Data Rates | 54, 48, 36, 24, 18, 12, 11, 9, 6, 5.5, 2, 1 Mbps
General
Operating Systems | Windows XP, 2000
Wi-FiŽ Alliance certification | Wi-FiŽ certification for 802.11b, 802.11g, 802.11a
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA, WPA-Enterprise, AES 128-bit, WEP 128-bit and 64-bit.Cisco Compatible Extensions v2.0, 802.1x
Product Safety | UL, C-UL, CB (IEC 60590)

Back to Contents

Trademarks and Disclaimers